Noris Medical Digital Analog

A. Update your 3Shape library with the attached *.dme file.

B: Analog Test Matrix: 
is designed to support you with choosing the right fit according to your printer.

Since each 3D printer has its own tolerance, we have developed a tool that will help you find out which settings of our library will
yield the best results for you.

Please follow the instructions below in order to choose the right settings.
This procedure is usually done once per printer.

1) Print the attached "MU/IH Analog Test" in your printer.

2) Check the fitting of the physical analog inside the matrix and find your desirable tolerance.

3) Go to the "Dental System Control Panel", under "Implant System"
   find "Noris Medical - Multi Unit/Internal Hex" library, and edit the "Abutment kits"
   following the number of the pleased fitting in the matrix.

4) Design your case using Model creator as usual.


For any additional information,
please E-mail us at digital@norismedical.com, and we should answer to you promptly.